{"text_format":"2","workbook":"xls","n_sheets":3,"sheets":["Sheet1","Sheet2","Sheet3"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":0,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Sheet1","index":0,"n_rows":142,"n_cols":5,"rows_kept":142,"cut":false,"hidden":false,"merged":[[0,0,0,4]],"flags":["formulas_cached_only"]}
["應施檢驗電機類商品實施型式認可檢驗品目明細表"]
["編號","商品分類號列","品      名","電器安規檢驗標準","電磁相容檢驗標準"]
[1,"6301.10.00.00.2","電毯（限檢驗300V以下，非屬藥事法所稱醫療器材者）","CNS 3765（94年版）、IEC 60335-2-81（2002-10）、IEC 60335-2-17（2002-10）、IEC 60335-2-23（2003-10）","CNS 13783-1（93年版）"]
[2,"6307.90.90.90.1F","其他製成之紡織品（限檢驗300V以下個人用之電保暖器具，非屬藥事法所稱醫療器材者）","CNS 3765（94年版）、IEC 60335-2-81（2002-10）、IEC 60335-2-17（2002-10）、IEC 60335-2-23（2003-10）","CNS 13783-1（93年版）"]
[3,"8414.51.00.00.2A","電風扇（限檢驗單相交流300V以下，未達125W者）","CNS 3765（94年版）、IEC 60335-2-80（2004-03）","CNS 13783-1（93年版）"]
[4,"8414.59.00.00.4A","電風扇（限檢驗單相交流300V以下，125W以上者）","CNS 3765（94年版）、IEC 60335-2-80（2004-03）","CNS 13783-1（93年版）"]
[5,"8414.60.00.00.1","含有風扇之通風罩或再循環罩，其最大水平邊長為不超過120公分者（限檢驗單相交流300V以下之排油煙機）","CNS 3765（94年版）、IEC 60335-2-31（2002-10）","CNS 13783-1（93年版）"]
[6,"8415.10.10.10.7","具有冷藏機組之窗型或壁型空氣調節器，自足式（限檢驗消耗功率在3千瓦以下者）","CNS 3765（94年版）、IEC 60335-2-40（2005-07）、CNS 3615（93年版，第4.6、4.7、4.8及4.9節暖氣性能部分暫不實施）","CNS 13783-1（93年版）"]
[7,"8415.10.10.20.5","具有冷藏機組之窗型或壁型空氣調節器，分離式系統（限檢驗消耗功率在3千瓦以下者）","CNS 3765（94年版）、IEC 60335-2-40（2005-07）、CNS 3615（93年版，第4.6、4.7、4.8及4.9節暖氣性能部分暫不實施）","CNS 13783-1（93年版）"]
[8,"8415.10.90.10.0","其它窗型或壁型空氣調節器，自足式（限檢驗消耗功率在3千瓦以下者）","CNS 3765（94年版）、IEC 60335-2-40（2005-07）、CNS 3615（93年版，第4.6、4.7、4.8及4.9節暖氣性能部分暫不實施）","CNS 13783-1（93年版）"]
[9,"8415.10.90.20.8","其它窗型或壁型空氣調節器，分離式系統（限檢驗消耗功率在3千瓦以下者）","CNS 3765（94年版）、IEC 60335-2-40（2005-07）、CNS 3615（93年版，第4.6、4.7、4.8及4.9節暖氣性能部分暫不實施）","CNS 13783-1（93年版）"]
[10,"8415.81.00.00.5A","箱型空氣調節器（限檢驗冷氣能力在26KW以下氣冷式或水冷式者）","CNS 3765（94年版）、IEC 60335-2-40（2005-07）、CNS 3615（93年版，第4.6、4.7、4.8及4.9節暖氣性能部分暫不實施）","CNS 13783-1（93年版）"]
[11,"8415.82.00.00.4A","箱型空氣調節器（限檢驗冷氣能力在26KW以下氣冷式或水冷式者）","CNS 3765（94年版）、IEC 60335-2-40（2005-07）、CNS 3615（93年版，第4.6、4.7、4.8及4.9節暖氣性能部分暫不實施）","CNS 13783-1（93年版）"]
[12,"8418.21.20.00.1","壓縮式家用冰箱容量在500公升及以上，但小於800公升者（限檢驗單相交流300V以下，有效內容積700公升以下者）","CNS 3765（94年版）、IEC 60335-2-24（2005-04）、CNS 2062（89年版）第5.2節『冷卻性能』、第5.3節『冷卻速度』、第5.10節『能源效率規定』及第7節『標示』","CNS 13783-1（93年版）"]
[13,"8418.21.90.00.6","其他壓縮式家用冰箱（限檢驗單相交流300V以下，有效內容積700公升以下者）","CNS 3765（94年版）、IEC 60335-2-24（2005-04）、CNS 2062（89年版）第5.2節『冷卻性能』、第5.3節『冷卻速度』、第5.10節『能源效率規定』及第7節『標示』","CNS 13783-1（93年版）"]
[14,"8418.22.90.00.5","其他電動吸收式家用冰箱（限檢驗單相交流300V以下，有效內容積700公升以下者）","CNS 3765（94年版）、IEC 60335-2-24（2005-04）","CNS 13783-1（93年版）"]
[15,"8418.29.90.00.8","其他形式家用冰箱（限檢驗單相交流300V以下，有效內容積700公升以下者）","CNS 3765（94年版）、IEC 60335-2-24（2005-04）、CNS 2062（89年版）第5.2節『冷卻性能』、第5.3節『冷卻速度』、第5.10節『能源效率規定』及第7節『標示』","CNS 13783-1"]
[16,"8418.40.00.00.2","直立式冷凍櫃，容量不超過900公升者（限檢驗單相交流300V以下，有效內容積400公升以下者）","CNS 3765（94年版）、IEC 60335-2-24（2005-04）、CNS 2062（89年版）第5.2節『冷卻性能』、第5.3節『冷卻速度』、第5.10節『能源效率規定』及第7節『標示』","CNS 13783-1"]
[17,"8418.50.00.00.9A","其他冷藏（保溫）箱（限檢驗300V以下，有效內容積100公升以下者）","CNS 3765（94年版）、IEC 60335-2-24（2005-04）","CNS 13783-1（93年版）"]
[18,"8418.69.90.00.9A","飲水供應機（限檢驗單相交流300V以下，含製冷裝置者）","CNS 3765（94年版）、IEC 60335-2-15（2005-08）、CNS 3910(89年版)第1.3節『輸出水溫』","CNS 13783-1（93年版）"]
[19,"8418.69.90.00.9B","開飲機（限檢驗單相交流300V以下，含製冷裝置者）（蒸餾水式飲水供應機列此號列）","CNS 3765（94年版）、IEC 60335-2-15（2005-08）、CNS 13516(89年版) 第4.10節『水溫』、第4.14節『生水阻隔裝置』、『構造』之第5.1.9節規定","CNS 13783-1（93年版）"]
[20,"8421.12.00.00.1","布料脫水機（限檢驗單相交流300V以下者）","CNS 3765（94年版）、IEC 60335-2-4（2005-01）","CNS 13783-1（93年版）"]
[21,"8421.39.10.00.8","電動空氣過濾器或電動空氣清潔器（限檢驗300V以下，非屬藥事法所稱醫療器材者）","CNS 3765（94年版）、IEC 60335-2-65（2005-09）","CNS 13783-1（93年版）"]
[22,"8422.11.00.00.1","家用洗碗碟機（限檢驗單相交流300V以下，額定消耗功率1KW以下者）","CNS 3765（94年版）、IEC 60335-2-5（2005-03）","CNS 13783-1（93年版）"]
[23,"8422.19.00.00.3","其他洗碗碟機（限檢驗單相交流300V以下，額定消耗功率1KW以下者）","CNS 3765（94年版）、IEC 60335-2-5（2005-03）","CNS 13783-1（93年版）"]
[24,"8450.11.10.00.4","全自動洗衣機，包括洗衣脫水兩用機，其容量為乾衣8公斤至10公斤者（限檢驗單相交流300V以下者）","CNS 3765（94年版）、IEC 60335-2-7（2004-11）","CNS 13783-1（93年版）"]
[25,"8450.11.20.00.2","全自動洗衣機，包括洗衣脫水兩用機，其容量為乾衣6公斤及以上，但未達8公斤者（限檢驗單相交流300V以下者）","CNS 3765（94年版）、IEC 60335-2-7（2004-11）","CNS 13783-1（93年版）"]
[26,"8450.11.30.00.0","全自動洗衣機，包括洗衣脫水兩用機，其容量為乾衣未達6公斤者（限檢驗單相交流300V以下者）","CNS 3765（94年版）、IEC 60335-2-7（2004-11）","CNS 13783-1（93年版）"]
[27,"8450.12.10.00.3","其他附有離心脫水槽之洗衣機，其容量為乾衣8公斤至10公斤者（限檢驗單相交流300V以下者）","CNS 3765（94年版）、IEC 60335-2-7（2004-11）","CNS 13783-1（93年版）"]
[28,"8450.12.20.00.1","其他附有離心脫水槽之洗衣機，其容量為乾衣6公斤及以上，但未達8公斤者（限檢驗單相交流300V以下者）","CNS 3765（94年版）、IEC 60335-2-7（2004-11）","CNS 13783-1（93年版）"]
[29,"8450.12.30.00.9","其他附有離心脫水槽之洗衣機，其容量為乾衣6公斤以下者（限檢驗單相交流300V以下者）","CNS 3765（94年版）、IEC 60335-2-7（2004-11）","CNS 13783-1（93年版）"]
[30,"8450.19.10.00.6","其他洗衣機，其容量為乾衣8公斤至10公斤者（限檢驗單相交流300V以下者）","CNS 3765（94年版）、IEC 60335-2-7（2004-11）","CNS 13783-1（93年版）"]
[31,"8450.19.20.00.4","其他洗衣機，其容量為乾衣6公斤以上，但未達8公斤者（限檢驗單相交流300V以下者）","CNS 3765（94年版）、IEC 60335-2-7（2004-11）","CNS 13783-1（93年版）"]
[32,"8450.19.30.00.2","其他洗衣機，其容量為乾衣未達6公斤者（限檢驗單相交流300V以下者）","CNS 3765（94年版）、IEC 60335-2-7（2004-11）","CNS 13783-1（93年版）"]
[33,"8450.20.00.00.5","洗衣機，包括洗衣、脫水兩用機，其容量為乾衣超過10公斤者（限檢驗單相交流300V以下者）","CNS 3765（94年版）、IEC 60335-2-7（2004-11）","CNS 13783-1（93年版）"]
[34,"8451.21.10.00.1","乾衣機，其容量為乾衣8公斤至10公斤者（限檢驗單相交流300V以下者）","CNS 3765（94年版）、IEC 60335-2-11（2002-03）+A1、IEC 60335-2-43（2002-10）","CNS 13783-1（93年版）"]
[35,"8451.21.20.00.9","乾衣機，其容量為乾衣6公斤及以上，但未達8公斤者（限檢驗單相交流300V以下者）","CNS 3765（94年版）、IEC 60335-2-11（2002-03）+A1、IEC 60335-2-43（2002-10）","CNS 13783-1（93年版）"]
[36,"8451.21.30.00.7","乾衣機，其容量為乾衣未達6公斤者（限檢驗單相交流300V以下者）","CNS 3765（94年版）、IEC 60335-2-11（2002-03）+A1、IEC 60335-2-43（2002-10）","CNS 13783-1（93年版）"]
[37,"8451.29.00.00.5","乾衣機，其容量為乾衣超過10公斤者（限檢驗單相交流300V以下者）","CNS 3765（94年版）、IEC 60335-2-11（2002-03）+A1、IEC 60335-2-43（2002-10）","CNS 13783-1（93年版）"]
[38,"8472.90.30.00.8","削鉛筆機（限檢驗單相交流300V以下之電動削鉛筆機，不含充電式）","CNS 14336","CNS 13783-1（93年版）"]
[39,"8479.89.10.00.8A","水涼（冷）扇（限檢驗水冷扇或水冷暖兩用式箱扇其電壓單相交流300V以下，額定消耗電功率：無電熱裝置者500W以下；有電熱裝置者：2KW以下）","CNS 3765（94年版）、IEC 60335-2-80（2004-03）、IEC 60335-2-30（2004-09）","CNS 13783-1（93年版）"]
[40,"8479.89.10.00.8B","除濕機（限檢驗單相交流300V以下，消耗電功率500W以下，具壓縮機式者）","CNS 3765（94年版）、IEC 60335-2-40（2005-07）、CNS 12492（89年版）","CNS 13783-1（93年版）"]
[41,"8504.10.00.00.3A","放電式燈泡或燈管之安定器（限檢驗螢光燈管用交流電子式安定器）","CNS 13755（95年版）、IEC 61347-1（2003-11）、61347-2-3（2004-09）+A1,A2"]
[42,"8504.10.00.00.3B","放電式燈泡或燈管之安定器（限檢驗預熱式熱陰極螢光燈管用之安定器）","CNS 927（95年版）、IEC 61347-1（2003-11）、61347-2-8（2006-03）"]
[43,"8509.10.00.00.8","家用電動真空吸塵器（限檢驗單相交流300V以下，不含充電式）","CNS 3765（94年版）、IEC 60335-2-2（2004-11）","CNS 13783-1（93年版）"]
[44,"8509.20.00.00.6","家用電動地板擦光器（含電動打臘機）（限檢驗單相交流300V以下，不含充電式）","CNS 3765（94年版）、IEC 60335-2-10（2002-10）","CNS 13783-1（93年版）"]
[45,"8509.40.00.00.2A","電動食品碾磨器（限檢驗單相交流300V以下者）","CNS 3765（94年版）、IEC 60335-2-14（2002-10）","CNS 13783-1（93年版）"]
[46,"8509.40.00.00.2B","電動食品混合器（檢驗範圍包括電動果汁機、絞肉機）（限檢驗單相交流300V以下者）","CNS 3765（94年版）、IEC 60335-2-14（2002-10）","CNS 13783-1（93年版）"]
[47,"8509.40.00.00.2C","電動榨汁機（限檢驗單相交流300V以下者）","CNS 3765（94年版）、IEC 60335-2-14（2002-10）","CNS 13783-1（93年版）"]
[48,"8509.40.00.00.2D","磨咖啡豆機（限檢驗單相交流300V以下，不含充電式）","CNS 3765（94年版）、IEC 60335-2-14（2002-10）","CNS 13783-1（93年版）"]
[49,"8509.80.90.00.4A","電捕昆蟲器（限檢驗單相交流300V以下，非以電氣方式滅昆蟲者）","CNS 3765（94年版）、IEC 60335-2-59（2002-10）","CNS 13783-1（93年版）"]
[50,"8509.80.90.00.4B","電動刨冰機（限檢驗單相交流300V以下，不含充電式）","CNS 3765（94年版）、IEC 60335-2-14（2002-10）","CNS 13783-1（93年版）"]
[51,"8509.80.90.00.4C","電動擦鞋機（限檢驗單相交流300V以下，不含充電式）","CNS 3765（94年版）","CNS 13783-1（93年版）"]
[52,"8509.80.90.00.4D","除濕機（限檢驗單相交流300V以下，消耗電功率500W以下，具壓縮機式者）","CNS 3765（94年版）、IEC 60335-2-40（2005-07）、CNS 12492（89年版）","CNS 13783-1（93年版）"]
[53,"8510.10.00.00.5","電鬍刀（限檢驗單相交流300V以下，不含充電式）","CNS 3765（94年版）、IEC 60335-2-8（2005-10）","CNS 13783-1（93年版）"]
[54,"8510.20.00.00.3","電剪髮器（限檢驗單相交流300V以下，不含充電式）","CNS 3765（94年版）、IEC 60335-2-8（2005-10）","CNS 13783-1（93年版）"]
[55,"8516.10.00.00.9A","即熱式電熱水器（限檢驗單相交流300V以下者）","CNS 3765（94年版）、IEC 60335-2-35（2002-10）","CNS 13783-1（93年版）"]
[56,"8516.10.00.00.9B","儲存式電熱水器（限檢驗單相交流300V以下者）","CNS 3765（94年版）、IEC 60335-2-21（2004-11）","CNS 13783-1（93年版）"]
[57,"8516.10.00.00.9C","儲備型電開水器（限檢驗單相250V、60A、500L以下）","CNS 3765（94年版）、IEC 60335-2-15（2005-08）","CNS 13783-1（93年版）"]
[58,"8516.10.00.00.9D","飲水供應機（不含製冷裝置者）（限檢驗單相交流300V以下者）","CNS 3765（94年版）、IEC 60335-2-15（2005-08）、CNS 3910(89年版)第1.3節『輸出水溫』","CNS 13783-1（93年版）"]
[59,"8516.10.00.00.9E","開飲機（不含製冷裝置者）（限檢驗單相交流300V以下者）（蒸餾水式飲水供應機列此號列）","CNS 3765（94年版）、IEC 60335-2-15（2005-08）、CNS 13516 (88年版)第4.10節『水溫』、第4.14節『生水阻隔裝置』、『構造』之第5.1.9節規定","CNS 13783-1（93年版）"]
[60,"8516.10.00.00.9F","浸入式電熱水器（限檢驗300V以下，3kW以下者）","CNS 3765（94年版）、IEC 60335-2-74（2003-03）＋am1（2006-04）","CNS 13783-1（93年版）"]
[61,"8516.21.00.00.6","儲熱式電暖器（限檢驗單相交流300V以下之一般家用電暖器）","CNS 3765（94年版）、IEC 60335-2-30（2004-09）、IEC 60335-2-61（2005-06）","CNS 13783-1（93年版）"]
[62,"8516.29.90.00.9","其他空間電加熱器（限檢驗單相交流300V以下之一般家用電暖器）","CNS 3765（94年版）、IEC 60335-2-30（2004-09）、IEC 60335-2-61（2005-06）","CNS 13783-1（93年版）"]
[63,"8516.31.00.00.4","乾髮器（限檢驗單相交流300V以下手持式）","CNS 3765（94年版）、 IEC 60335-2-23（2003-10）","CNS 13783-1（93年版）"]
[64,"8516.32.00.00.3A","其他美髮器具（限檢驗單相交流300V以下電梳）","CNS 3765（94年版）、 IEC 60335-2-23（2003-10）","CNS 13783-1（93年版）"]
[65,"8516.32.00.00.3B","其他美髮器具（限檢驗燙（整）髮機）","CNS 3765（94年版）、IEC 60335-2-23（2003-10）","CNS 13783-1（93年版）"]
[66,"8516.33.00.00.2","烘手機（限檢驗單相交流300V以下者）","CNS 3765（94年版）、 IEC 60335-2-23（2003-10）","CNS 13783-1（93年版）"]
[67,"8516.40.00.00.3A","電熨斗（限檢驗單相交流300V以下者）","CNS 3765（94年版）、IEC 60335-2-3（2005-01）","CNS 13783-1（93年版）"]
[68,"8516.40.00.00.3B","電動蒸氣熨斗（限檢驗單相交流300V以下者）","CNS 3765（94年版）、IEC 60335-2-3（2005-01）","CNS 13783-1（93年版）"]
[69,"8516.50.00.00.0","微波爐（限檢驗單相交流300V以下者）","CNS 3765（94年版）、IEC 60335-2-25（2005-06）","CNS 13803（92年版）"]
[70,"8516.60.10.00.6","電烤箱（限檢驗單相交流300V以下者）","CNS 3765（94年版）、IEC 60335-2-6（2005-04）、IEC 60335-2-9（2004-03）","CNS 13783-1（93年版）"]
[71,"8516.60.20.00.4","電鍋（包括炒鍋、燉鍋及電碗）（限檢驗單相交流300V以下者）","CNS 3765（94年版）、IEC 60335-2-13（2004-07）、IEC 60335-2-15（2005-08）","CNS 13783-1（93年版）"]
[72,"8516.60.30.00.2","電磁爐（限檢驗單相交流300V以下者）","CNS 3765（94年版）、IEC 60335-2-6（2005-04）、IEC 60335-2-9（2004-03）","CNS 13803"]
[73,"8516.60.90.00.9","其他烤箱，炊具，炊盤，煮環，烤器，烘焙器（限檢驗單相交流300V以下電烘烤爐）","CNS 3765（94年版）、IEC 60335-2-6（2005-04）、IEC 60335-2-9（2004-03）","CNS 13783-1（93年版）"]
[74,"8516.71.00.00.5A","電壺（限檢驗單相交流300V以下者）","CNS 3765（94年版）、IEC 60335-2-15（2005-08）、電熱水瓶產品須再符合 CNS 12625(82年版) 第4.4.2節『異常溫度』、第4.10節『水溫』規定","CNS 13783-1（93年版）"]
[75,"8516.71.00.00.5B","電濾煮器（電咖啡壺）（限檢驗單相交流300V以下，額定消耗功率3KW以下者）","CNS 3765（94年版）、IEC 60335-2-15（2005-08）","CNS 13783-1（93年版）"]
[76,"8516.71.00.00.5C","電咖啡機（限檢驗單相交流300V以下，額定消耗功率3KW以下，烘、磨、濾煮一體或磨、濾煮一體之電咖啡機）","CNS 3765（94年版）、IEC 60335-2-15（2005-08）、IEC 60335-2-14（2002-10）","CNS 13783-1（93年版）"]
[77,"8516.72.00.00.4","烤麵包器（限檢驗單相交流300V以下者）","CNS 3765（94年版）、IEC 60335-2-9（2004-03）","CNS 13783-1（93年版）"]
[78,"8516.79.00.00.7A","電爐（限檢驗單相交流300V以下者）","CNS 3765（94年版）、IEC 60335-2-6（2005-04）、IEC 60335-2-9（2004-03）","CNS 13783-1（93年版）"]
[79,"8516.79.00.00.7B","電烤肉餅器（限檢驗單相交流300V以下者）","CNS 3765（94年版）、IEC 60335-2-9（2004-03）","CNS 13783-1（93年版）"]
[80,"8516.79.00.00.7F","電灶（限檢驗單相交流300V以下，消耗電功率在10KW以下者）","CNS 3765（94年版）、IEC 60335-2-6（2005-04）","CNS 13783-1（93年版）"]
[81,"8516.79.00.00.7G","電熱式烘碗機（限檢驗單相交流300V以下者）","CNS 3765（94年版）、IEC 60335-2-5（2005-03）","CNS 13783-1（93年版）"]
[82,"8516.79.00.00.7H","電熱夾式烤盤（限檢驗單相交流300V以下，消耗電功率在3KW以下者）","CNS 3765（94年版）、IEC 60335-2-9（2004-03）","CNS 13783-1（93年版）"]
[83,"8516.79.00.00.7J","被服烘乾機（限檢驗單相交流300V以下者）","CNS 3765（94年版）、IEC 60335-2-43（2002-10）","CNS 13783-1（93年版）"]
[84,"8516.79.00.00.7K","魚缸加溫器（限檢驗單相交流300V以下額定消耗功率1KW以下者）","CNS 3765（94年版）、IEC 60335-2-55（2002-11）","CNS 13783-1（93年版）"]
[85,"8516.79.00.00.7L","保溫盤（限檢驗單相交流300V以下額定消耗功率1KW以下者）","CNS 3765（94年版）、IEC 60335-2-12（2002-10）","CNS 13783-1（93年版）"]
[86,"8516.79.00.00.7M","電蚊香器（限檢驗單相交流300V以下者）","CNS 3765（94年版）","CNS 13783-1（93年版）"]
[87,"8516.79.00.00.7N","電芳香器（限檢驗單相交流300V以下者）","CNS 3765（94年版）","CNS 13783-1（93年版）"]
[88,"8516.79.00.00.7O","電熱便當箱（限檢驗單相交流300V以下，額定消耗功率1KW以下者）","CNS 3765（94年版）、IEC 60335-2-6（2005-04）","CNS 13783-1（93年版）"]
[89,"8516.79.00.00.7P","電氣蒸籠（限檢驗單相交流300V以下，額定消耗功率1KW以下者）","CNS 3765（94年版）、IEC 60335-2-15（2005-08）、IEC 60335-2-6（2005-04）","CNS 13783-1（93年版）"]
[90,"8516.79.00.00.7Q","保溫鍋（限檢驗單相交流300V以下，額定消耗功率1KW以下者）","CNS 3765（94年版）、IEC 60335-2-15（2005-08）","CNS 13783-1（93年版）"]
[91,"8516.79.00.00.7R","保溫箱（限檢驗單相交流300V以下，額定消耗功率1KW以下者）","CNS 3765（94年版）、IEC 60335-2-6（2005-04）、IEC 60335-2-9（2004-03）","CNS 13783-1（93年版）"]
[92,"8516.79.00.00.7S","保溫壺（限檢驗單相交流300V以下，額定消耗功率1KW以下者）","CNS 3765（94年版）、IEC 60335-2-15（2005-08）","CNS 13783-1（93年版）"]
[93,"8516.79.00.00.7T","奶瓶消毒器（限檢驗單相交流300V以下，額定消耗功率1KW以下者）","CNS 3765（94年版）、IEC 60335-2-15（2005-08）","CNS 13783-1（93年版）"]
[94,"8516.79.00.00.7U","蒸（煮）蛋器（限檢驗單相交流300V以下，額定消耗功率1KW以下者）","CNS 3765（94年版）、IEC 60335-2-15（2005-08）","CNS 13783-1（93年版）"]
[95,"8516.79.00.00.7V","個人用之電保暖器具（限檢驗300V以下，非屬藥事法所稱醫療器材者）","CNS 3765（94年版）、IEC 60335-2-81（2002-10）、IEC 60335-2-17（2002-10）、IEC 60335-2-23（2003-10）","CNS 13783-1（93年版）"]
[96,"8522.90.30.30.2","錄影帶用迴帶機（限檢驗單相交流300V以下者）","CNS 3765（94年版）","CNS 13783-1（93年版）"]
[97,"8531.80.10.00.3","電鈴（限檢驗交流電壓300V以下之各種電鈴）","CNS 8799"]
[98,"8536.10.00.00.5","熔絲裝置，電壓未超過1000V者（限檢驗300V以下低壓電力配線用熔線）","CNS 2225、2226、2227"]
[99,"8536.20.41.00.4","無熔絲開關，電壓未超過1000V者，電流超過600A者（限檢驗使用於電壓600V以下，額定電流800A以下，啟斷容量220V/50kA以下者）","CNS 14816-2或IEC 60947-2"]
[100,"8536.20.49.00.6","其他無熔絲開關，電壓未超過1000V者（限檢驗使用於電壓600V以下，額定電流800A以下，啟斷容量220V/50kA以下者）","CNS 14816-2或IEC 60947-2、IEC 60898"]
[101,"8536.20.90.00.4","其他自動斷路器，電壓未超過1000V者，（限檢驗交流電壓600V以下，額定電流225A以下之漏電斷路器）","CNS 5422或IEC 61008-1、IEC 61009-1"]
[102,"8536.50.90.00.7A","家用配線用開關（限檢驗300V以下者）","CNS 695或IEC 60669-1"]
[103,"8536.50.90.00.7B","閘刀開關（限檢驗300V以下者）","CNS 1488、696"]
[104,"8536.69.90.00.6A","配線用插頭及插座（限檢驗300V以下者）","CNS 690或IEC 60884-2-5或IEC 60884-1＋CNS 690極形"]
[105,"8536.69.90.00.6B","器具用插頭及插座（限檢驗300V以下者）","CNS 6797或IEC 60320-1或IEC 60320-1＋CNS 6797極形"]
[106,"8539.31.00.00.7A","熱陰極螢光燈管（泡）（限檢驗一般照明用低壓交流預熱起動型直管式、環管式及瞬時起動型螢光燈管）","CNS 691"]
[107,"8539.31.00.00.7B","熱陰極螢光燈管（泡）（限檢驗安定器內藏式螢光燈泡）","CNS 14125"]
[108,"8543.89.30.00.6","臭氧產生器（限檢驗300V以下之電動空氣過濾器或電動空氣清潔器，非屬藥事法所稱醫療器材者）","CNS 3765（94年版）、IEC 60335-2-65（2005-09）","CNS 13783-1（93年版）"]
[109,"8543.89.99.90.5A","電捕昆蟲器（限檢驗單相交流300V以下，以電氣方式滅昆蟲者）","CNS 3765（94年版）、IEC 60335-2-59（2002-10）","CNS 13783-1（93年版）"]
[110,"8544.51.90.00.6","其他電源線及線組，裝有插接器，電壓超過80V，但未超過1000V者（限檢驗300V以下之一般電源線組）","CNS 10917、10917-1、10917-2、10917-3或IEC 60799"]
[111,"8544.59.90.00.8B","聚氯乙烯絕緣電力電纜","CNS 3301、6556或IEC 60227"]
[112,"8544.59.90.00.8G ","聚氯乙烯絕緣電線","CNS 679或IEC 60227"]
[113,"8544.59.90.00.8H","橡膠絕緣電線","CNS 675或IEC 60245"]
[114,"8544.59.90.00.8J","橡膠花線","CNS 546或IEC 60245"]
[115,"8544.59.90.00.8K","聚氯乙烯（PVC）花線","CNS 3199或IEC 60227"]
[116,"8544.59.90.00.8L","引出用橡膠絕緣電線","CNS 5747或IEC 60245"]
[117,"8544.59.90.00.8M","電機器具用聚氯乙烯絕緣電線","CNS 6070或IEC 60227"]
[118,"8544.59.90.00.8N","耐熱聚氯乙烯絕緣電線","CNS 8379或EC 60227"]
[119,"8544.59.90.00.8O","屋外用聚氯乙烯絕緣電線","CNS 8559或IEC 60227"]
[120,"8544.59.90.00.8P","聚乙烯絕緣電線","CNS 10314或IEC 60227"]
[121,"8544.59.90.00.8Q","聚氯乙烯絕緣接戶電線","CNS 7781或IEC 60227"]
[122,"8544.59.90.00.8R","橡膠絕緣輕便電纜","CNS 10741、10599或IEC 60245"]
[123,"9019.10.19.00.8","其他理療按摩器具（限檢驗單相交流300V以下之手提式按摩器，不含充電式）","CNS 3765（94年版）、IEC 60335-2-32（2002-10）","CNS 13783-1（93年版）"]
[124,"9404.21.00.00.9","泡沫橡膠或塑膠製褥，不論有無外罩者（限檢驗300V以下之電熱褥，非屬藥事法所稱醫療器材者）","CNS 3765（94年版）、IEC 60335-2-81（2002-10）、IEC 60335-2-17（2002-10）、IEC 60335-2-23（2003-10）","CNS 13783-1（93年版）"]
[125,"9404.29.00.10.9","紡織材料製褥（限檢驗300V以下之電熱褥，非屬藥事法所稱醫療器材者）","CNS 3765（94年版）、IEC 60335-2-81（2002-10）、IEC 60335-2-17（2002-10）、IEC 60335-2-23（2003-10）","CNS 13783-1（93年版）"]
[126,"9404.29.00.90.2","其他材料製褥（限檢驗300V以下之電熱褥，非屬藥事法所稱醫療器材者）","CNS 3765（94年版）、IEC 60335-2-81（2002-10）、IEC 60335-2-17（2002-10）、IEC 60335-2-23（2003-10）","CNS 13783-1（93年版）"]
[127,"9404.30.00.00.8","睡袋（限檢驗300V以下個人用之電保暖器具，非屬藥事法所稱醫療器材者）","CNS 3765（94年版）、IEC 60335-2-81（2002-10）、IEC 60335-2-17（2002-10）、IEC 60335-2-23（2003-10）","CNS 13783-1（93年版）"]
[128,"9404.90.10.00.3","蓋被褥（限檢驗300V以下之電熱褥，非屬藥事法所稱醫療器材者）","CNS 3765（94年版）、IEC 60335-2-81（2002-10）、IEC 60335-2-17（2002-10）、IEC 60335-2-23（2003-10）","CNS 13783-1（93年版）"]
[129,"9404.90.20.00.1","床罩（床單）（限檢驗300V以下之電熱褥，非屬藥事法所稱醫療器材者）","CNS 3765（94年版）、IEC 60335-2-81（2002-10）、IEC 60335-2-17（2002-10）、IEC 60335-2-23（2003-10）","CNS 13783-1（93年版）"]
[130,"9404.90.90.11.3","其他寢具及類似家具，羊毛製（限檢驗300V以下個人用之電保暖器具，非屬藥事法所稱醫療器材者）","CNS 3765（94年版）、IEC 60335-2-81（2002-10）、IEC 60335-2-17（2002-10）、IEC 60335-2-23（2003-10）","CNS 13783-1（93年版）"]
[131,"9404.90.90.19.5","其他寢具及類似家具，其他紡織材料製（限檢驗300V以下個人用之電保暖器具，非屬藥事法所稱醫療器材者）","CNS 3765（94年版）、IEC 60335-2-81（2002-10）、IEC 60335-2-17（2002-10）、IEC 60335-2-23（2003-10）","CNS 13783-1（93年版）"]
[132,"9404.90.90.90.7","其他寢具及類似家具，其他材料製（限檢驗300V以下個人用之電保暖器具，非屬藥事法所稱醫療器材者）","CNS 3765（94年版）、IEC 60335-2-81（2002-10）、IEC 60335-2-17（2002-10）、IEC 60335-2-23（2003-10）","CNS 13783-1（93年版）"]
[133,"9405.10.00.00.1","枝形吊燈及其他天花板或牆壁之電照明配件，不包括公共場所或街道照明用者（限檢驗一般室內照明用者）","CNS 14335、IEC 60598-2-1、IEC 60598-2-2、IEC 60598-2-6、IEC 60598-2-23","CNS 14115（93年版）"]
[134,"9405.20.00.00.9A","檯、桌、床邊或落地之電燈具（限檢驗交流300V以下之熱陰極螢光燈桌上檯燈）","CNS 14335、IEC 60598-2-4（1994）","CNS 14115（93年版）"]
[135,"9405.20.00.00.9B","檯、桌、床邊或落地之電燈具（限檢驗其他檯、桌、床邊或落地之燈具）","CNS 14335、IEC 60598-2-4、IEC 60598-2-6","CNS 14115（93年版）"]
[136,"9405.30.00.00.7","耶誕樹用燈串（限檢驗交流300V以下之燈串組）","CNS 14335、IEC 60598-2-20（1996）＋A1"]
[137,"9405.40.50.00.4","礦工燈（限檢驗安全帽燈）","CNS 2415"]
[138,"9405.40.90.00.6B","其他電燈具及照明配件（限檢驗一般室內照明用者）","CNS 14335、IEC 60598-2-1、IEC 60598-2-2、IEC 60598-2-6、IEC 60598-2-23","CNS 14115"]
[139,"9405.40.90.00.6C","神明桌用神明燈","CNS 14335（88年版）、IEC 60598-2-1（1979-01）＋am1（1987-01）、IEC 60598-2-2（1996-05）＋am1（1997-01）、IEC 60598-2-4（1997-04）、IEC 60598-2-6（1994-06）＋am1（1996-11）、IEC 60598-2-23（1996-04）＋am1（2000-05）","CNS 14115（93年版）"]
[140,"9405.60.00.20.6A","安全標誌燈","CNS 9648、10207、10208"]

{"sheet":"Sheet2","index":1,"n_rows":0,"n_cols":0,"rows_kept":0,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}

{"sheet":"Sheet3","index":2,"n_rows":0,"n_cols":0,"rows_kept":0,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}